1.Click "Connect device" to make sure device is connected.If success, the dmdtype is showed.
2.Click to choose file.
	If the dmdtype is "XGA_07A" or "XGA_055A", the dmd is 1024x768.
		Please select *.bin in Pictrue_1024 floder.
	If the dmdtype is "1080P_095A", the dmd is 1920x1080.
		Please select *.bin in Picture_1920 floder.

3.the 1920x1080 only support gray 1, please don't select other.	

4.Click start.